Agency USEP (2014) Food Waste Management in the United States. Office of Resource Conservation and Recovery. Available at [https://www.epa.gov/sites/production/files/2016-12/documents/food\_waste\_management\_2014\_12082016\_508.pdf. Accessed 21st Jan 2021](https://www.epa.gov/sites/production/files/2016-12/documents/food_waste_management_2014_12082016_508.pdf.%20Accessed%2021st%20Jan%202021)

Ali Shah F, Mahmood Q, Maroof Shah M, Pervez A, Ahmad Asad S (2014) Microbial ecology of anaerobic digesters: the key players of anaerobiosis. Sci World J. <https://doi.org/10.1155/2014/183752>

Dhar H, Kumar P, Kumar S, Mukherjee S, Vaidya AN (2016) Effect of organic loading rate during anaerobic digestion of municipal solid waste. Bioresour Technol 217:56–61. <https://doi.org/10.1016/j.biortech.2015.12.004>

Haider MR, Yousaf S, Malik RN, Visvanathan C (2015) Effect of mixing ratio of food waste and rice husk co-digestion and substrate to inoculum ratio on biogas production. Bioresour Technol 190:451–457. <https://doi.org/10.1016/j.biortech.2015.02.105>

Luo K, Pang Y, Yang Q, Wang D, Li X, Lei M, Huang Q (2019) A critical review of volatile fatty acids produced from waste activated sludge: enhanced strategies and its applications. Environ Sci Pollut Res 26:13984–13998. <https://doi.org/10.1007/s11356-019-04798-8>

Meegoda JN, Li B, Patel K, Wang LB (2018) A review of the processes, parameters, and optimization of anaerobic digestion. Int J Environ Res Public Health 15:2224. <https://doi.org/10.3390/ijerph15102224>

Motte J-C, Escudié R, Hamelin J, Steyer J-P, Bernet N, Delgenes J-P, Dumas C (2014) Substrate milling pretreatment as a key parameter for solid-state anaerobic digestion optimization. Bioresour Technol 173:185–192. <https://doi.org/10.1016/j.biortech.2014.09.015>